


Topology.




1.config rip.


2. Config ospf










Show ip route










Loopback









Show ip route for R2





Similarly do for R1 you may face some disturbance while typing

Show ip route for R2



Ping 40.0.0.0 from 10.0.0.10

